; xxx and xxxNamexxx are placeholder which have to be filled in.
; all preset data is derived from the IX1 PROFIBUS DP slave firmware and
; should not be changed.
; The name of this File (NAMExxxx.GSD) consits of 4 characters (NAME), in 
; general the abbreviation of the vendor name, and the 4 Ident_Number 
; digits (xxxx).
;
;=========================================================================
; KPFA00DB.GSD
; GSD-file for PFA700
; Vendor:			G. Kromschröder AG 
; GSD-file date:		10.09.98 
;=========================================================================
;
#Profibus_DP 
GSD_Revision           = 1                      ; Version 
Vendor_Name            = "G. Kromschröder AG"	; (max. 32 char)
Model_Name             = "PFA700"       	; device name (max. 32 char)
Revision               = "1.0"			; device revision (max. 32 char)
Ident_Number           = 0x00DB			; UINT16, e.g. 0x1A2B (hex)
;
Protocol_Ident         = 0	                ; Protokollkennung 0=DP-Geraet
Station_Type           = 0	                ; Geraetetyp 0=Slave,1=Master
FMS_supp               = 0	                ; Mischgeraet 0=nur DP, 1=DP/FMS
;
Hardware_Release       = "1.0"	                ; (max. 32 char)
Software_Release       = "V2.4"	                ; (max. 32 char)
;
; device supports (=1) following baudrates:
9.6_supp               = 1
19.2_supp              = 1
93.75_supp             = 1
187.5_supp             = 1
500_supp               = 1
1.5M_supp              = 1
;
; device has following 'max station delay responder' times [Tbit]
MaxTsdr_9.6            = 60
MaxTsdr_19.2           = 60
MaxTsdr_93.75          = 60
MaxTsdr_187.5          = 60
MaxTsdr_500            = 100
MaxTsdr_1.5M           = 150
;
Repeater_Ctrl_Sig      = 0
24V_Pins               = 0
Implementation_Type    = "ANDERER"
;
; device supports following PROFIBUS DP slave services
Freeze_Mode_supp       = 1
Sync_Mode_supp         = 1
Auto_Baud_supp         = 1
Set_Slave_Add_supp     = 0
;
User_Prm_Data_Len      = 0
Max_Diag_Data_Len      = 6
Min_Slave_Intervall    = 1                      ; unit [100us]	
;
Slave_Family           = 2
;
Modular_Station        = 0                      ; compact device (no modular device)
Modul_Offset           = 0
Max_Module             = 1
Max_Input_Len          = 5
Max_Output_Len         = 3
Max_Data_Len           = 8
;
; device configuration, use hex codes for configuration_data bytes, 
; example:   Module    = "digital 8 bit output, 24 bit input" 0x20, 0x12
Module                 = "24 Bit Output, 40 Bit Input" 0x22, 0x14
EndModule
